|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1 | 1 | Each | **GENERAL CONDITIONS:**1. All items to be delivered and installed FOB:

 OSU Institute1801 East 4th Street Okmulgee, OK 744471. Brand and model of equipment being quoted must be shown.
2. An “or equal” item must meet or exceed the requirements listed on these pages and a detailed brochure and specifications must accompany quote response.
3. Warranty information should be sent with quote response.
4. Flag Pole to be fully complete for flying of flags upon installation.
5. Installation must be scheduled with OSU Institute of Technology Physical Plant Services.
6. Days required for installation ARO: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Architectural Aluminum Commercial Tapered Flag Poles** Furnish all equipment, labor, materials and supplies to deliver and install flag poles on the OSU Institute of Technology campus as specified below. Flag pole, Liberty Flags Item # IHEL508188B or equal.Pole to be duranodic bronze to match existing window casing on the Grady clack Student Success Center. The installation to include:Exposed height: 50’ erectedButt Diameter: 10”Top Diameter: 4”.188” Wall thickness (minimum)Color/Finish: Duranodic Bronze/Brushed SatinGold Ball FinialConcealed internal halyard systemRevolving Truck (pulley), winch mounted inside shaftSolid Braided Nylon Halyard/ropeChrome Plated Snap HooksSteel Ground SleeveCast Aluminum CleatFlash CollarWind speed: 95 MPH flagged 1 Year Warranty (minimum)

|  |  |
| --- | --- |
|  |  |

Brand \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Model \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Warranty \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | $\_\_\_\_\_\_\_\_\_\_ | $\_\_\_\_\_\_\_\_ |